**ASSIGNMENT 8: CUSTOM AT COMMANDS- C16QS**

|  |  |  |
| --- | --- | --- |
| **Command** | **Purpose** | **Mock Response** |
| AT+CAVSTATUS? | Returns module's overall connectivity state | +CAVSTATUS: Registered, Signal=20, IP=Yes OK |
| AT+CAVRESET | Reboots the module | +CAVRESET: Rebooting... OK |
| AT+CAVFWVER? | Fetches firmware version of the module | +CAVFWVER: C16QS\_R02.05.01\_2405 OK |